## Settings to generate MSC file
# Configuration from SPI Flash as per XAPP1233
set_property BITSTREAM.GENERAL.COMPRESS TRUE [current_design]
set_property BITSTREAM.CONFIG.EXTMASTERCCLK_EN DIV-1 [current_design]
set_property BITSTREAM.CONFIG.SPI_32BIT_ADDR YES [current_design]
set_property BITSTREAM.CONFIG.SPI_BUSWIDTH 8 [current_design]
set_property BITSTREAM.CONFIG.SPI_FALL_EDGE YES [current_design]
# Set CFGBVS to GND to match schematics
set_property CFGBVS GND [current_design]
# Set CONFIG_VOLTAGE to 1.8V to match schematics
set_property CONFIG_VOLTAGE 1.8 [current_design]
# Set safety trigger to power down FPGA at 125degC
set_property BITSTREAM.CONFIG.OVERTEMPSHUTDOWN Enable [current_design]

