CAPI=2:

name : :microwatt:litesdcard:0

generators:
  litesdcard_gen:
    interpreter: python3
    command: fusesoc-add-files.py
    description: Generate a litesdcard SD-card controller
    usage: |
      litesdcard_gen adds the pre-generated LiteX LiteSDCard SD-card controller
      based on the vendor type.

      Parameters:
        vendor: The vendor type (xilinx)
